CORNERSTONE DRC checklist

Top cell: Performed by: Date:

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Item** | **Checked** | | | | | | | | | | | |
| **GDS 303** | **GDS 304** | **GDS**  **98** |  |  |  |  |  |  |  |  |  |
| Minimum feature size |  |  |  |  |  |  |  |  |  |  |  |  |
| Minimum gap |  |  |  |  |  |  |  |  |  |  |  |  |
| Correct design area used |  | | | | | | | | | | | |
| Waveguides extend correctly into bleed region |  | | | | | | | | | | | |
| Labels layer does not overlap with waveguide layer |  | | | | | | | | | | | |
| Feature edges are smooth (correct field grid used) |  | | | | | | | | | | | |