CORNERSTONE DRC checklist

Top cell: Performed by: Date:

|  |  |
| --- | --- |
| **Item** | **Checked** |
| **GDS 303** | **GDS 304** | **GDS****98** |  |  |  |  |  |  |  |  |  |
| Minimum feature size  |  |  |  |  |  |  |  |  |  |  |  |  |
| Minimum gap |  |  |  |  |  |  |  |  |  |  |  |  |
| Correct design area used |  |
| Waveguides extend correctly into bleed region |  |
| Labels layer does not overlap with waveguide layer |  |
| Feature edges are smooth (correct field grid used) |  |